{"text_format":"1","workbook":"xlsx","n_sheets":26,"sheets":["91-ID3(TH-37)","91-ID3 chart (H-25)","91-ID4(H-38)","91-ID4 chart(H-26)","91-ID6(TH-39)","91-ID6 chart(T-27)","91-ID7(TH-40)","91-ID7 chart(H-28)","94-IDC-1(TH-41)","94-IDC-1 chrt(-29)","96-1(TH-42)","96-1 chrt(H-30)","96-2(TH-43)","96-2chrt(H-31)","96-3(A&B)(TH-44)","96-3 chrt (A+B)(H-32)","96-4(ABC&D)(TH-45)","96-4 chrt (A,B,C+D)(H-33)","P01-03A(TH-46)","P01-03 chrt(H-34)","P01-04(A&B)(Th-47)","P01-04(H-35)","BKS04-06(TH-48)","BKS04-06(H-36) ","BKS04-07(TH-49)","BKS04-07(H-37)"],"not_rendered":{"charts":26,"images":2,"macros":0,"external_links":0,"defined_names":17,"comments":5,"pivot_tables":0},"unopened":[{"sheet":"91-ID3 chart (H-25)","index":1,"reason":"not_a_worksheet"},{"sheet":"91-ID4 chart(H-26)","index":3,"reason":"not_a_worksheet"},{"sheet":"91-ID6 chart(T-27)","index":5,"reason":"not_a_worksheet"},{"sheet":"91-ID7 chart(H-28)","index":7,"reason":"not_a_worksheet"},{"sheet":"94-IDC-1 chrt(-29)","index":9,"reason":"not_a_worksheet"},{"sheet":"96-1 chrt(H-30)","index":11,"reason":"not_a_worksheet"},{"sheet":"96-2chrt(H-31)","index":13,"reason":"not_a_worksheet"},{"sheet":"96-3 chrt (A+B)(H-32)","index":15,"reason":"not_a_worksheet"},{"sheet":"96-4 chrt (A,B,C+D)(H-33)","index":17,"reason":"not_a_worksheet"},{"sheet":"P01-03 chrt(H-34)","index":19,"reason":"not_a_worksheet"},{"sheet":"P01-04(H-35)","index":21,"reason":"not_a_worksheet"},{"sheet":"BKS04-06(H-36) ","index":23,"reason":"not_a_worksheet"},{"sheet":"BKS04-07(H-37)","index":25,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"91-ID3(TH-37)","index":0,"n_rows":53,"n_cols":13,"rows_kept":53,"cut":false,"hidden":false,"merged":[[52,0,52,1],[51,0,51,6],[0,0,1,1],[0,4,0,5],[1,4,1,5],[2,4,2,5],[3,6,4,6],[3,0,4,0],[3,5,4,5],[3,1,3,2],[3,3,3,4]]}
["BH91-ID3",null,"Location:","Intermediate Dam South \nAbutment @ Stn. 0+810","Shallow Tip \nElevation (m amsl):",null,1036.82]
[null,null,"Coordinates:","8V580359 \n6913723","Deep Tip \nElevation (m amsl):",null,1028.6199999999999]
["Surface Protector:","yes","Date Installed:",1991,"2004 Surface\nElevation (m amsl):",null,1043.82]
["Date"," Reading                                                              (psi)",null,"Piezometric Elevation \n(m amsl)",null,"Pond El.\n(m amsl)","Comments",null,null,"Date"]
[null,"Shallow","Deep","Shallow","Deep",null,null,null,null,null,"Surface Elevation","Shallow Tip Elevation","Deep Tip Elevation"]
["1991-07-01",1.2285714285712857,9.7142857142856496,{"$f":"1036.82+B6*0.7","v":1037.6799999999998},{"$f":"1028.62+C6*0.7","v":1035.4199999999998},1042.2,null,null,null,"1991-07-01",1043.82,1036.82,1028.6199999999999]
["1991-08-01",4.2857142857103882E-2,9.3999999999998973,{"$f":"1036.82+B7*0.7","v":1036.8499999999999},{"$f":"1028.62+C7*0.7","v":1035.1999999999998},1042.2,null,null,null,"2012-12-25",1043.82,1036.82,1028.6199999999999]
["1991-09-01",null,8.5999999999999748,{"$f":"1036.82+B8*0.7","v":1036.82},1034.6399999999999,1042.2]
["1992-02-01"]
["1992-04-01"]
["1992-06-01",3.4428571428569352,13.457142857142962,{"$f":"1036.82+B11*0.7","v":1039.2299999999998},1038.04,1047.7]
["1992-09-01",1.0999999999999741,10.514285714285572,1037.5899999999999,1035.9799999999998,1047.7]
["1994-05-01",0.1999999999998181,10.7,1036.9599999999998,1036.1099999999999,1047.7]
["1994-09-01",0.39999999999996105,9.0999999999998451,1037.0999999999999,1034.9899999999998,1047.7]
["1995-09-01",0,9.5000000000001297,1036.82,1035.27,1047.7]
["1996-10-01",0.1,7.5,1036.8899999999999,1033.8699999999999,1048.0999999999999]
["1997-05-07",0.2,6.4,1036.96,1033.0999999999999]
["1997-10-17",0.4,8.31,1037.0999999999999,1034.4369999999999]
["1998-05-27",0.1,11.7,1036.8899999999999,1036.81,1048.0999999999999]
["1998-11-12",0.22,7.1,1036.9739999999999,1033.5899999999999,1047.8]
["1998-12-16",0,6.3,1036.82,1033.03,1047.8]
["1999-05-29",0.4,11.05,1037.0999999999999,1036.3549999999998,1048]
["1999-09-16",0.02,8.4,1036.8339999999998,1034.5,1047.7]
["2000-06-14",0.01,10.41,1036.827,1035.9069999999999,1047.5999999999999]
["2000-09-09",0,9.5,1036.82,1035.27]
["2001-06-10",0.1,10.3,1036.8899999999999,1035.83]
["2001-09-20",0.01,8.1999999999999993,1036.827,1034.3599999999999]
["2002-06-18",0,9.1,1036.82,1034.9899999999998]
["2002-09-10",0,8.1999999999999993,1036.82,1034.3599999999999]
["2002-11-04",0,7.1,1036.82,1033.5899999999999]
["2002-11-10",0,6.5,1036.82,1033.1699999999998]
[{"$f":"'P01-03A(TH-46)'!A9","v":"2003-06-11"},0.2,8.6999999999999993,1036.96,1034.7099999999998,null,"*have to continue using old piezometer, tips are too big"]
[{"$f":"'P01-03A(TH-46)'!A10","v":"2003-09-10"},0,6.3,1036.82,1033.03,null,"* Installed new tips, now using new box"]
["2004-05-10",0,5.2,1036.82,1032.26,null,"2004 survey data used from this point on"]
["2004-07-19",0,6.2,1036.82,1032.9599999999998]
["2004-09-09",0.1,5.7,1036.8899999999999,1032.6099999999999]
["2005-05-26",0,8.4,{"$f":"1036.82+B37*0.7","v":1036.82},{"$f":"1028.62+C37*0.7","v":1034.5}]
["2005-09-14",0,4.9000000000000004,1036.82,1032.05]
["2006-03-09",0,3.3,1036.82,1030.9299999999998]
["2006-03-27",0.1,3.4,1036.8899999999999,1031]
["2006-06-14",0.1,7.1,1036.8899999999999,1033.5899999999999]
["2006-10-02",0.1,4.0999999999999996,1036.8899999999999,1031.4899999999998]
["2007-05-22",0,4.5999999999999996,{"$f":"1036.82+B43*0.7","v":1036.82},{"$f":"1028.62+C43*0.7","v":1031.8399999999999},1046.7809999999999,"Good Flow "]
["2007-09-26",0.1,5.7,1036.8899999999999,1032.6099999999999]
["2008-09-24",0.1,6.1,1036.8899999999999,1032.8899999999999,1046.1969999999999]
["2009-06-29",0.1,5.7,1036.8899999999999,1032.6099999999999]
["2009-09-30",0.2,5.3,1036.96,1032.33,1046.048]
["2010-05-15",0.2,5.2,1036.96,1032.26,1046.269]
["2010-06-02",1,7.9,1037.52,1034.1499999999999,1045.94]
["2010-08-04",0.1,3.4,1036.8899999999999,1031,1044.2850000000001]
["2010-09-10",10.1,3.1,1043.8899999999999,1030.79,1043.7260000000001]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]
["Note: Check results"]

{"sheet":"91-ID4(H-38)","index":2,"n_rows":57,"n_cols":13,"rows_kept":57,"cut":false,"hidden":false,"merged":[[56,0,56,2],[55,0,55,6],[0,0,1,1],[0,4,0,5],[1,4,1,5],[2,4,2,5],[3,6,5,6],[3,0,5,0],[3,5,5,5],[3,1,3,2],[3,3,3,4]]}
["BH91-ID4",null,"Location:","Intermediate Dam \nToe @St.0+567","Shallow Tip \nElevation (m amsl):",null,1024.22]
[null,null,"Coordinates:","8V580517 \n6913926","Deep Tip \nElevation (m amsl):",null,1017.08]
["Surface Protector:","yes","Date Installed:",1991,"*Surface \nElevation (m amsl):",null,1031.8]
["Date"," Reading                                                              (psi)",null,"Piezometric Elevation\n(m amsl)",null,"Pond El.\n(m amsl)","Comments",null,null,"Date"]
[null,"Shallow","Deep","Shallow","Deep",null,null,null,null,null,"Surface Elevation","Shallow Tip Elevation","Deep Tip Elevation"]
[null,"(upper)","(lower)","(upper)","(lower)",null,null,null,null,"1991-07-01",1031.8,1024.22,1017.08]
["1991-07-01",10.342857142857156,19.05714285714274,1031.46,1030.42,1042.2,null,null,null,"2011-12-31",1031.8,1024.22,1017.08]
["1991-08-01",10.814285714285624,19.199999999999754,1031.79,1030.52,1042.2]
["1991-09-01",11.1,19.3,1031.99,1030.5899999999999,1042.2]
["1992-02-01",12.242857142857053,19.585714285714015,1032.79,1030.79,1047.7]
["1992-04-01",12.442857142857196,19.642857142857142,1032.93,1030.83,1047.7]
["1992-06-01",14.800000000000184,20.399999999999999,1034.58,1031.3599999999999,1047.7]
["1992-09-01",11.857142857142794,21.1,1032.52,1031.8499999999999,1047.7]
["1994-05-01",10,18.699999999999886,1031.22,1030.17,1047.7]
["1994-09-01",8.900000000000027,17.399999999999768,1030.45,1029.26,1047.7,null,null,null,33420]
["1995-09-01",11.000000000000066,18.999999999999936,1031.92,1030.3800000000001,1047.7,null,null,null,38353]
["1996-09-01",10,null,1031.22,null,1048.0999999999999]
["1996-10-01",9.6999999999999993,18.8,1031.01,1030.24]
["1997-05-07",6.3,null,1028.6300000000001]
["1997-10-17",11.58,null,1032.326]
["1998-05-27",11.04,null,1031.9480000000001,null,1048.0999999999999]
["1998-08-07",null,19.399999999999999,null,1030.6600000000001,1048.0999999999999]
["1998-11-12",9.2200000000000006,null,1030.674,null,1047.8]
["1998-12-04",8.6999999999999993,18,1030.31,1029.68,1047.8]
["1999-05-29",11.4,20,1032.2,1031.08,1048]
["1999-09-16",7.7,16.2,1029.6099999999999,1028.42,1047.7]
["2000-06-14",10.5,19.100000000000001,1031.57,1030.45,1047.5999999999999]
["2000-09-09",9.8000000000000007,18.2,1031.08,1029.82]
["2001-06-10",9.5,18.100000000000001,1030.8699999999999,1029.75]
["2001-09-20",9.6999999999999993,18.2,1031.01,1029.82]
["2002-06-18",9.6999999999999993,18.8,1031.01,1030.24]
["2002-09-10",9,17.8,1030.52,1029.54]
["2002-11-04",9,17.600000000000001,1030.52,1029.4000000000001]
["2002-11-10",9.1999999999999993,17.7,1030.6600000000001,1029.47]
[{"$f":"'P01-03A(TH-46)'!A9","v":"2003-06-11"},9,17.7,1030.52,1029.47,null,"*New piezometer readout used"]
[{"$f":"'P01-03A(TH-46)'!A10","v":"2003-09-10"},7.6,16.399999999999999,1029.54,1028.56]
["2004-05-10",8.9,18.100000000000001,1030.45,1029.75,null,"No 2004 elevation data"]
["2004-07-19",9.1999999999999993,17.8,1030.6600000000001,1029.54]
["2004-09-09",8.6,17.2,1030.24,1029.1199999999999]
["2005-05-26",7.5,16,1029.47,1028.28]
["2005-09-14",6.5,15.1,1028.77,1027.6500000000001]
["2006-03-09",5.9,14.5,{"$f":"$G$1+B42*0.7","v":1028.3500000000001},{"$f":"$G$2+C42*0.7","v":1027.23}]
["2006-03-27",6.3,14.9,1028.6300000000001,1027.51]
["2006-06-14",6.3,14.9,1028.6300000000001,1027.51]
["2006-10-02",6.3,14.9,1028.6300000000001,1027.51]
["2007-05-22",8.1999999999999993,16.8,1029.96,1028.8400000000001,1046.7809999999999,"Good Flow "]
["2007-09-26",5.8,15,1028.28,1027.58]
["2008-05-20",9.1999999999999993,17.5,1030.6600000000001,1029.33]
["2008-06-11",8.6999999999999993,16.899999999999999,1030.31,1028.9100000000001]
["2008-09-24",7.9,16.399999999999999,{"$f":"$G$1+B50*0.7","v":1029.75},{"$f":"$G$2+C50*0.7","v":1028.56},1046.1969999999999]
["2009-06-29",6.7,15.2,1028.9100000000001,1027.72]
["2009-09-30",8.6999999999999993,16.899999999999999,1030.31,1028.9100000000001,1046.048]
["2010-05-15",8.4,16.899999999999999,1030.1000000000001,1028.9100000000001,1046.269]
["2010-06-02",16.7,13.8,1035.9100000000001,1026.74,1045.94]
["2010-09-10",6.7,14.6,1028.9100000000001,1027.3,1043.7260000000001]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]
["Note: Check results"]

{"sheet":"91-ID6(TH-39)","index":4,"n_rows":58,"n_cols":15,"rows_kept":58,"cut":false,"hidden":false,"merged":[[57,0,57,2],[3,6,5,6],[0,3,0,4],[1,3,1,4],[2,3,2,4],[56,0,56,7],[0,0,1,1],[3,0,5,0],[3,1,5,1],[3,4,3,5],[3,2,3,3],[0,5,0,6],[1,5,1,6],[2,5,2,6],[3,7,5,7]]}
["BH91-ID6",null,"Location:","Intermediate Dam Toe  \n@St.0+630",null,"Shallow Tip \nElevation (m amsl):",null,1024.8]
[null,null,"Coordinates:","8V580475 \n6913866",null,"Deep Tip Elevation \n(m amsl):",null,1016.9]
["Surface Protector:","yes","Date Installed:",1991,null,"2004 Surface \nElevation (m amsl):",null,1031.3599999999999]
["Date",null," Reading                                                              (psi)",null,"Piezometric Elevation\n(m amsl)",null,"Pond El. \n(m amsl)","Comments",null,null,null,"Date"]
[null,null,"Shallow","Deep","Shallow","Deep",null,null,null,null,null,null,"Surface Elevation","Shallow Tip Elevation","Deep Tip Elevation"]
[null,null,"(upper)","(lower)","(upper)","(lower)",null,null,null,null,null,"1991-07-01",1031.3599999999999,1024.8,1016.9]
["1991-07-01",null,7.8857142857142604,20.328571428571458,1030.32,1031.1300000000001,1042.2,null,null,null,null,"2011-12-31",1031.3599999999999,1024.8,1016.9]
["1991-08-01",null,8.0571428571430008,20.914285714285533,1030.44,1031.54,1042.2]
["1991-09-01",null,8.2000000000000135,20.799999999999923,1030.54,1031.46,1042.2]
["1992-02-01",null,8.2000000000000135,20.7,1030.54,1031.3900000000001,1047.7]
["1992-04-01",null,9.0571428571430648,23.099999999999781,1031.1400000000001,1033.07,1047.7]
["1992-06-01",null,9.9142857142857927,25.799999999999923,1031.74,1034.96,1047.7]
["1992-09-01",null,8.6714285714288053,21.357142857142925,1030.8699999999999,1031.8499999999999,1047.7]
["1994-05-01",null,7.2000000000002737,20,1029.8399999999999,1030.9000000000001,1047.7]
["1994-09-01",null,6.200000000000208,18.899999999999999,1029.1400000000001,1030.1300000000001,1047.7]
["1995-09-01",null,7.5,20,1030.05,1030.9000000000001,1047.7]
["1996-09-01",null,6.6,null,1029.42,null,1048.0999999999999]
["1996-10-01",null,5.8,21.1,1028.8599999999999,1031.67]
["1997-05-07",null,2.9,null,1026.83]
["1997-10-17",null,8.41,null,1030.6869999999999]
["1998-05-27",null,8.56,null,1030.7919999999999,null,1048.0999999999999]
["1998-08-07",null,null,20.8,null,1031.46,1048.0999999999999]
["1998-11-12",null,6.57,null,1029.3989999999999,null,1047.8]
["1998-12-04",null,6.8,19.5,1029.56,1030.55,1047.8]
["1999-05-29",null,8.7799999999999994,21.5,1030.9459999999999,1031.95,1048]
["1999-09-16",null,5.3,17.600000000000001,1028.51,1029.22,1047.7]
["2000-06-14",null,7.7,20.41,1030.19,1031.1870000000001,1047.5999999999999]
["2000-09-09",null,6.8,19.7,1029.56,1030.69]
["2001-06-10",null,6.8,19.5,1029.56,1030.55]
["2001-09-20",null,7,19.7,1029.7,1030.69]
["2002-06-18",null,6.8,19.600000000000001,1029.56,1030.6199999999999]
["2002-09-10",null,6.5,19.2,1029.3499999999999,1030.3399999999999]
["2002-11-04",null,6.3,19,1029.21,1030.2]
["2002-11-10",null,6.3,19.2,1029.21,1030.3399999999999]
[{"$f":"'P01-03A(TH-46)'!A9","v":"2003-06-11"},null,6.4,19,1029.28,1030.2,null,"*New piezometer started use here"]
[{"$f":"'P01-03A(TH-46)'!A10","v":"2003-09-10"},null,5.0999999999999996,17.600000000000001,1028.3699999999999,1029.22]
["2004-05-10",null,6.3,19,{"$f":"1024.8+C37*0.7","v":1029.21},{"$f":"1016.9+D37*0.7","v":1030.2},null,"2004 survey data used from this point on"]
["2004-07-19",null,6.5,19.100000000000001,1029.3499999999999,1030.27]
[{"$f":"'91-ID3(TH-37)'!A36","v":"2004-09-09"},null,5.9,18.600000000000001,1028.93,1029.92]
[{"$f":"'91-ID3(TH-37)'!A37","v":"2005-05-26"},null,4.5,17.399999999999999,1027.95,1029.08]
[{"$f":"'91-ID3(TH-37)'!A38","v":"2005-09-14"},null,3.6,16.5,1027.32,1028.45]
["2006-03-09",null,3.5,16.100000000000001,1027.25,1028.17]
["2006-03-27",null,3.4,16.399999999999999,1027.18,1028.3799999999999,null,"3.4/3.5 won't stabilize"]
["2006-06-14",null,3.7,16.3,1027.3899999999999,1028.31]
["2006-10-02",null,3.5,16.3,1027.25,1028.31]
["2007-05-22",null,5.4,18.100000000000001,{"$f":"1024.8+C46*0.7","v":1028.58},{"$f":"1016.9+D46*0.7","v":1029.57},1046.7809999999999,"Good flow "]
["2007-09-26",null,3.6,16.600000000000001,1027.32,1028.52]
["2008-05-20",null,6.1,18.899999999999999,1029.07,1030.1299999999999]
["2008-06-11",null,5.7,18.399999999999999,1028.79,1029.78]
["2008-09-24",null,5.2,17.899999999999999,1028.44,1029.43,1046.1969999999999]
["2009-06-29",null,3.9,16.600000000000001,1027.53,1028.52]
["2009-09-15",null,4.8,"n/r",{"$f":"1024.8+C52*0.7","v":1028.1599999999999}]
["2009-09-30",null,5.5,18.5,{"$f":"1024.8+C53*0.7","v":1028.6499999999999},1029.8499999999999,1046.048]
["2010-05-15",null,5.6,18.3,{"$f":"1024.8+C54*0.7","v":1028.72},1029.71,1046.269]
["2010-06-02",null,23,5.6,{"$f":"1024.8+C55*0.7","v":1040.8999999999999},1020.8199999999999,1045.94]
["2010-09-10",null,3.3,16,{"$f":"1024.8+C56*0.7","v":1027.1099999999999},1028.0999999999999,1043.7260000000001]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]
["Note: Check results"]

{"sheet":"91-ID7(TH-40)","index":6,"n_rows":53,"n_cols":11,"rows_kept":53,"cut":false,"hidden":false,"merged":[[0,0,1,1],[0,3,0,4],[52,0,52,5]]}
["BH91-ID7",null,"Location:","Intermediate Dam Toe  @St.0+759"]
[null,null,"Coordinates:","8V580377 \n6913751","Tip Elevation \n(m amsl):",1025.95]
["Surface Protector:","yes","Date Installed:",1991,"2004 Ground\nElevation (amsl):",1032.42]
["Date",null," Reading (psi)","Piezometric \nElevation\n(m amsl)","Pond El. \n(m amsl)","Comments",null,null,"Date"]
["1991-07-01",null,8.9428571428571306,1032.21,1042.2,null,null,null,null,"Surface Elevation","Tip Elevation"]
["1991-08-01",null,9.0571428571427415,1032.29,1042.2,null,null,null,"1991-07-01",1032.42,1025.95]
["1991-09-01",null,8.900000000000027,1032.18,1042.2,null,null,null,"2012-12-31",1032.42,1025.95]
["1992-02-01",null,13.214285714285715,1035.2,1047.7]
["1992-04-01",null,10.014285714285702,1032.96,1047.7]
["1992-06-01",null,10.614285714285806,1033.3800000000001,1047.7]
["1992-09-01",null,9.2142857142857792,1032.4000000000001,1047.7]
["1994-05-01",null,8.5999999999999748,1031.97,1047.7]
["1994-09-01",null,7.4000000000000918,1031.1300000000001,1047.7]
["1995-09-01",null,8.9999999999999361,1032.25,1047.7]
["1996-09-01",null,8.1,1031.6199999999999,1048.0999999999999]
["1997-05-07",null,5.0999999999999996,1029.52]
["1997-10-17",null,9.36,1032.502]
["1998-05-27",null,9.49,1032.5930000000001,1048.0999999999999]
["1998-11-12",null,7.56,1031.242,1047.8]
["1998-12-16",null,7.6,1031.27,1047.8]
["1999-05-29",null,9.6,1032.67,1048]
["1999-09-16",null,6.6,1030.57,1047.7]
["2000-06-14",null,8.9,1032.18,1047.5999999999999]
["2000-09-09",null,7.5,1031.2]
["2001-06-10",null,8.1999999999999993,1031.69]
["2001-09-20",null,8.1,1031.6199999999999]
["2002-06-18",null,8.3000000000000007,1031.76]
["2002-09-10",null,7.7,1031.3399999999999]
["2002-11-04",null,7.5,1031.2]
["2002-11-10",null,7.4,1031.1300000000001]
[{"$f":"'P01-03A(TH-46)'!A9","v":"2003-06-11"},null,7.7,1031.3399999999999,null,"*New piezometer started use here"]
[{"$f":"'P01-03A(TH-46)'!A10","v":"2003-09-10"},null,6.2,1030.29]
["2004-05-10",null,7.2,{"$f":"$F$2+C33*0.7","v":1030.99},null,"2004 survey data used from here on"]
["2004-07-19",null,7.4,1031.1300000000001]
[{"$f":"'91-ID3(TH-37)'!A36","v":"2004-09-09"},null,6.9,1030.78]
[{"$f":"'91-ID3(TH-37)'!A37","v":"2005-05-26"},null,6.1,1030.22]
[{"$f":"'91-ID3(TH-37)'!A38","v":"2005-09-14"},null,5.0999999999999996,1029.52]
["2006-03-09",null,4.5999999999999996,1029.17]
["2006-03-27",null,4.8,1029.31]
["2006-06-14",null,5.4,1029.73]
["2006-10-02",null,4.9000000000000004,1029.3800000000001]
["2007-05-22",null,6.3,1030.3600000000001,1046.7809999999999,"Good Flow "]
["2007-09-26",null,5.5,1029.8]
["2008-05-20",null,7.3,1031.06]
["2008-06-11",null,6.9,1030.78]
["2008-09-24",null,6.4,{"$f":"$F$2+C46*0.7","v":1030.43},1046.1969999999999]
["2009-06-29",null,5.3,1029.6600000000001]
["2009-09-15",null,5.8,1030.01]
["2009-09-30",null,6.5,1030.5,1046.048]
["2010-05-15",null,6.5,1030.5,1046.269]
["2010-06-02",null,5.8,1030.01,1045.94]
["2010-09-10",null,4.3,1028.96,1043.7260000000001]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]

{"sheet":"94-IDC-1(TH-41)","index":8,"n_rows":44,"n_cols":14,"rows_kept":44,"cut":false,"hidden":false,"merged":[[0,0,1,1],[43,0,43,5]]}
["BH94-IDC-1",null,"Location:","Intermediate Dam Crest","2004 Stick Up (m):",0.27]
[null,null,"Coordinates:","8V580605 \n6913969","2004 Surface \nElevation (m amsl):",1049.21]
["Surface Protector:","Yes","Date Installed:",1994,"Tip Elevation:","N/A"]
[]
["Date",null,"Water level from top of pipe                (m)","Piezometric Elevation \n(m amsl)","Pond El.  \n(m amsl)","Comments"]
["1994-06-02",null,null,null,1047.7,"dry",null,null,null,null,null,"Ground Surface","Bottom of Slotted Section","Top of Slotted Section"]
["1994-09-16",null,null,null,1047.7,"dry",null,null,null,null,"1990-09-01",1049.21,1035.46,{"$f":"C$2-7.78","v":{"$error":"#VALUE!"}}]
["1995-09-22",null,null,null,1047.7,"dry",null,null,null,null,"2010-12-31",1049.21,1035.46,{"$f":"N7","v":{"$error":"#VALUE!"}}]
["1996-09-25",null,null,null,1048.0999999999999,"dry"]
["1998-05-28",null,null,null,1048.0999999999999,"dry"]
["1998-11-13",null,14.1,1035.48,1047.8,"dry"]
["1999-06-08",null,14.1,1035.48,1047.8,"dry"]
["1999-09-16",null,14.18,1035.4000000000001,1047.7,"dry"]
["2000-06-14",null,14.11,1035.47,1047.5999999999999,"dry"]
["2000-09-09",null,14.11,1035.47,1047.5999999999999,"H2O"]
["2001-06-10",null,14.11,1035.47,1047.5999999999999]
["2001-08-01",null,14.11,1035.47,1047.5999999999999,"dry"]
["2002-06-18",null,14.11,1035.47,null,"dry"]
["2002-08-05",null,14.185,1035.395,null,"dry"]
["2002-09-02",null,14.11,1035.47,null,"dry"]
["2002-11-02",null,14.11,1035.47,null,"dry"]
["2002-11-10",null,14.11,1035.47,null,"dry"]
[{"$f":"'P01-03A(TH-46)'!A9","v":"2003-06-11"},null,14.12,1035.46,null,"dry"]
[{"$f":"'P01-03A(TH-46)'!A10","v":"2003-09-10"},null,14.11,1035.47,null,"dry"]
["2003-05-10",null,14.11,1035.47,null,"dry"]
["2004-07-19",null,14.11,{"$f":"$F$2+$F$1-C26","v":1035.3700000000001},null,"dry"]
[{"$f":"'91-ID3(TH-37)'!A36","v":"2004-09-09"},null,14.11,1035.3700000000001,null,"dry"]
[{"$f":"'91-ID3(TH-37)'!A37","v":"2005-05-26"},null,14.12,1035.3600000000001,null,"bottom"]
[{"$f":"'91-ID3(TH-37)'!A38","v":"2005-09-14"},null,14.12,1035.3600000000001,null,"bottom"]
["2006-03-09",null,14.17,1035.31]
["2006-03-27",null,14.13,1035.3499999999999,null,"no beep, ice crystals"]
["2006-06-14",null,14.125,1035.355,null,"bottom"]
["2006-10-02",null,14.12,1035.3600000000001]
["2007-05-22",null,14.135,1035.345,1046.7809999999999,"bottom and beep"]
["2007-09-26",null,14.125,1035.355,null,"no beep"]
["2008-05-20",null,14.15,1035.33,null,"no beep"]
["2008-06-11",null,14.14,1035.3399999999999,null,"no beep"]
["2008-09-24",null,14.14,{"$f":"$F$2+$F$1-C38","v":1035.3399999999999},1046.1969999999999,"no beep"]
["2009-06-29",null,14.15,1035.33,null,"no beep"]
["2009-09-30",null,14.154999999999999,1035.325,1046.048,"no beep"]
["2010-05-15",null,14.172000000000001,1035.308,1046.269,"no beep"]
["2010-06-02",null,14.15,1035.33,1045.94,"no beep"]
["2010-09-10",null,14.15,1035.33,1043.7260000000001,"no beep"]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation \nReview; 2010 Data compiled by DES"]

{"sheet":"96-1(TH-42)","index":10,"n_rows":56,"n_cols":14,"rows_kept":56,"cut":false,"hidden":false,"merged":[[0,0,1,1],[0,3,0,4],[55,0,55,5]]}
["BH96-1",null,"Location:","Intermediate Dam Crest"]
[null,null,"Coordinates:","8V580563 \n6913908","2004 Stick Up:",0.68]
["Surface Protector:","yes","Date Installed:",1996,"2004 Surface \nElevation (m amsl):",1049.1500000000001]
[null,null,"Screened Interval \n(m bgs):","18.77 - 21.80","Tip Elevation \n(m amsl):",1027.3499999999999,null,null,null,null,null,"Ground Surface","Bottom of Slotted Section","Top of Slotted Section"]
["Date",null,"Water level from top of pipe (m)",null,"Piezometric Elevation                             (m amsl)","Comments",null,null,null,null,"1996-01-01",1049.1500000000001,1027.3499999999999,1030.3800000000001]
["1996-09-08",null,20.059999999999999,null,1029.99,null,null,null,null,null,"2012-12-31",1049.1500000000001,1027.3499999999999,1030.3800000000001]
["1996-09-26"]
["1996-09-27"]
["1997-05-13"]
["1997-06-06"]
["1997-07-11"]
["1997-10-07",null,18.77,null,1031.28]
["1998-06-01",null,18.73,null,1031.32]
["1998-10-31",null,20.079999999999998,null,1029.97]
["1998-11-13",null,19.97,null,1030.08]
["1999-06-08",null,18.399999999999999,null,1031.6500000000001]
["1999-06-19"]
["1999-07-03"]
["1999-10-29",null,20.55,null,1029.5]
["1999-10-31"]
["2000-05-31"]
["2000-06-27"]
["2000-07-25"]
["2000-09-21",null,20.13,null,1029.92]
["2000-10-10"]
["2001-06-06"]
["2001-07-15"]
["2001-09-05"]
["2002-06-18"]
["2002-08-05",null,20.48,null,1029.57]
["2002-09-10",null,20.02,null,1030.03]
["2002-11-04",null,20.14,null,1029.9100000000001]
["2002-11-10",null,20.059999999999999,null,1029.99]
[{"$f":"'P01-03A(TH-46)'!A9","v":"2003-06-11"},null,20.024999999999999,null,1030.0250000000001]
[{"$f":"'P01-03A(TH-46)'!A10","v":"2003-09-10"},null,20.96,null,1029.0899999999999]
["2004-05-12",null,19.925000000000001,null,{"$f":"F$3+F$2-C36","v":1029.9050000000002},"2004 survey data used from here on"]
["2004-07-08",null,19.695,null,1030.1350000000002]
["2004-07-19",null,19.945,null,1029.8850000000002]
[{"$f":"'91-ID3(TH-37)'!A36","v":"2004-09-09"},null,20.324999999999999,null,1029.5050000000001,"clear"]
[{"$f":"'91-ID3(TH-37)'!A37","v":"2005-05-26"},null,21.17,null,1028.6600000000001,"ice"]
[{"$f":"'91-ID3(TH-37)'!A38","v":"2005-09-14"},null,21.82,null,1028.0100000000002]
["2006-03-09"]
["2006-03-27",null,null,null,null,"no read, frozen"]
["2006-06-14",null,2.27,null,null,"likely a mistake"]
["2006-10-02",null,21.98,null,1027.8500000000001]
["2007-05-22",null,null,null,null,"no read, frozen"]
["2007-09-26",null,21.655000000000001,null,1028.1750000000002]
["2008-05-20",null,1.22,null,null,"no beep, frozen "]
["2008-06-11",null,1.2,null,null,"no beep, frozen "]
["2008-09-24",null,20.97,null,1028.8600000000001]
["2009-06-29",null,3.08,null,null,"frozen"]
["2009-09-30",null,20.591000000000001,null,1029.2390000000003]
["2010-05-15",null,20.588999999999999,null,1029.2410000000002,"slush present"]
["2010-06-02",null,21.018000000000001,null,1028.8120000000001]
["2010-09-10",null,22.2,null,1027.6300000000001]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]

{"sheet":"96-2(TH-43)","index":12,"n_rows":55,"n_cols":12,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,3,0,4],[0,0,1,1],[54,0,54,5]]}
["BH96-2",null,"Location:","Intermediate Dam Crest"]
[null,null,"Coordinates:","8V580696 6914096","Tip Elevation\n(m amsl):",1028.8699999999999]
["Surface Protector:","yes","Date Installed:",1996,"2004 Surface Elevation:\n(m amsl)",1049.22]
[null,null,"Screened Interval (m bgs):","17.13 - 20.12","2004 Stick Up (m):",0.72]
["Date",null,"Water level from top of pipe (m)",null,"Piezometric Elevation                             (m amsl)","Comments",null,null,null,"Ground Surface","Bottom of Slotted Section","Top of Slotted Section"]
["1996-09-08",null,19.739999999999998,null,1030.31,null,null,null,"1996-01-01",1049.22,1028.8699999999999,1031.8599999999999]
["1996-09-26",null,null,null,null,null,null,null,"2012-12-31",1049.22,1028.8699999999999,1031.8599999999999]
["1996-09-27",null,19.940000000000001,null,1030.1099999999999]
["1997-05-13"]
["1997-06-06"]
["1997-07-11"]
["1997-10-07",null,18.3,null,1031.75]
["1998-06-01",null,18.440000000000001,null,1031.6099999999999]
["1998-10-31",null,19.8,null,1030.25]
["1998-11-13",null,19.690000000000001,null,1030.3599999999999]
["1999-06-08",null,18.11,null,1031.94]
["1999-06-19"]
["1999-07-03"]
["1999-10-29",null,20.25,null,1029.8]
["1999-10-31"]
["2000-05-31"]
["2000-06-27"]
["2000-07-25"]
["2000-09-21",null,19.78,null,1030.27]
["2000-10-10"]
["2001-06-06"]
["2001-07-15"]
["2001-09-05"]
["2002-06-18",null,19.375,null,1030.675]
["2002-08-05",null,20.149999999999999,null,1029.9000000000001]
["2002-09-10",null,19.68,null,1030.3699999999999]
["2002-11-04",null,19.815000000000001,null,1030.2349999999999]
["2002-11-10",null,19.73,null,1030.32]
[{"$f":"'P01-03A(TH-46)'!A9","v":"2003-06-11"},null,19.71,null,1030.3399999999999]
[{"$f":"'P01-03A(TH-46)'!A10","v":"2003-09-10"},null,20.65,null,1029.4000000000001]
["2004-05-10",null,21.07,null,{"$f":"F$3+F$4-C36","v":1028.8700000000001},"Dry reading, 2004 survey data used from here on"]
["2004-07-19",null,19.614999999999998,null,1030.325]
[{"$f":"'91-ID3(TH-37)'!A36","v":"2004-09-09"},null,20.02,null,1029.92]
[{"$f":"'91-ID3(TH-37)'!A37","v":"2005-05-26"},null,19.95,null,1029.99]
[{"$f":"'91-ID3(TH-37)'!A38","v":"2005-09-14"},null,21.04,null,1028.9000000000001,"bottom iron mud on probe"]
["2006-03-09",null,21.15,null,1028.79]
["2006-03-27",null,21.03,null,1028.9100000000001,"no beep, mud on probe"]
["2006-06-14",null,13.05]
["2006-10-02",null,21.04,null,1028.9000000000001]
["2007-05-22",null,20.34,null,1029.6000000000001,"no beep, dry"]
["2007-09-26",null,21.4,null,{"$f":"F$3+F$4-C46","v":1028.54}]
["2008-05-20",null,19.885000000000002,null,1030.0550000000001]
["2008-06-11",null,20.190000000000001,null,1029.75]
["2008-09-24",null,20.58,null,1029.3600000000001]
["2009-06-29",null,21.5,null,1028.44,"no beep"]
["2009-09-30",null,20.238,null,1029.702]
["2010-05-15",null,20.268999999999998,null,{"$f":"F$3+F$4-C52","v":1029.671}]
["2010-06-02",null,20.666,null,{"$f":"F$3+F$4-C53","v":1029.2740000000001}]
["2010-09-10",null,21.035,null,{"$f":"F$3+F$4-C54","v":1028.905}]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]

{"sheet":"96-3(A&B)(TH-44)","index":14,"n_rows":57,"n_cols":11,"rows_kept":57,"cut":false,"hidden":false,"merged":[[0,0,1,1],[5,5,6,5],[5,1,5,2],[5,0,6,0],[56,0,56,5]]}
["BH96-3",null,"Location:","Intermediate Dam Toe, \nnear the North Abutment","2004 Stick Up - A (m):",0.65]
[null,null,"Coordinates:","8V580529 \n6913934","2004 Stick Up - B (m):",0.59]
["Surface Protector:","yes","Date Installed:",1996,"2004 Surface \nElevation (m amsl):",1031.48]
[null,null,"Tip Elevation - A \n(m amsl):",1022.43,"Screened Interval - A \n(m bgs):","7.44 - 8.97"]
[null,null,"Tip Elevation - B \n(m amsl):",1012.23,"Screened Interval - B \n(m bgs):","17.7 - 19.17"]
["Date","Water level from top of pipe                                                        (m)",null,"Piezometric Elevation \n(m amsl)",null,"Comments",null,null,"Ground Surface","Tip A","Tip B"]
[null,"A","B","96-3A (Shallow)","96-3B   (Deep)",null,null,"1996-01-01",1031.48,1022.51,1012.31]
["1996-09-08",2.37,2.25,1029.71,1029.78,null,null,"2012-12-31",1031.48,1022.51,1012.31]
["1996-09-26",2.5299999999999998,2.4,1029.55,1029.6300000000001]
["1996-09-27"]
["1997-05-13",4.5,4.32,1027.58,1027.71]
["1997-06-06"]
["1997-07-11"]
["1997-10-07",1.06,0.95,1031.02,1031.08]
["1998-06-01",1.07,0.99,1031.01,1031.04]
["1998-10-31",2.44,2.34,1029.6400000000001,1029.69]
["1998-11-13"]
["1999-06-08"]
["1999-06-19",0.7,0.57999999999999996,1031.3800000000001,1031.45]
["1999-07-03"]
["1999-10-29",2.94,2.82,1029.1400000000001,1029.21]
["1999-10-31"]
["2000-05-31"]
["2000-06-27",2.41,2.2599999999999998,1029.67,1029.77]
["2000-07-25"]
["2000-09-21"]
["2000-10-10",2.2000000000000002,2.0499999999999998,1029.8800000000001,1029.98]
["2001-06-06",2.38,2.2400000000000002,1029.7,1029.79]
["2001-07-15",2,1.86,1030.08,1030.17]
["2001-09-05",1.98,1.86,1030.0999999999999,1030.17]
["2002-06-18",1.81,null,1030.27]
["2002-08-05"]
["2002-09-10",2.5649999999999999,2.42,1029.5150000000001,1029.6099999999999]
["2002-11-04"]
["2002-11-10"]
[{"$f":"'96-2(TH-43)'!A34","v":"2003-06-11"},2.4700000000000002,2.34,1029.6099999999999,1029.69]
[{"$f":"'96-2(TH-43)'!A35","v":"2003-09-10"},3.43,3.28,1028.6500000000001,1028.75]
["2004-07-08",2.15,2.0099999999999998,{"$f":"F$3+F$1-B38","v":1029.98},{"$f":"F$3+F$2-C38","v":1030.06},"2004 survey data used from here on"]
["2004-07-19",2.4,2.2250000000000001,1029.73,1029.845]
[{"$f":"'91-ID3(TH-37)'!A36","v":"2004-09-09"},2.77,2.645,1029.3600000000001,1029.425,"clear, sulphur smell"]
[{"$f":"'91-ID3(TH-37)'!A37","v":"2005-05-26"},3.66,3.49,1028.47,1028.58]
[{"$f":"'91-ID3(TH-37)'!A38","v":"2005-09-14"},4.3650000000000002,4.18,1027.7650000000001,1027.8899999999999]
["2006-03-09",4.76,4.59,1027.3700000000001,1027.48]
["2006-03-27",4.43,4.26,1027.7,1027.81]
["2006-06-14",4.45,4.26,1027.68,1027.81]
["2006-10-02",4.42,4.3,1027.71,1027.77]
["2007-05-22",2.29,2.88,{"$f":"F$3+F$1-B47","v":1029.8400000000001},{"$f":"F$3+F$2-C47","v":1029.1899999999998},"a- frozen no beep"]
["2007-09-26",4.0599999999999996,3.94,1028.0700000000002,1028.1299999999999]
["2008-05-20",2.56,2.48,1029.5700000000002,1029.5899999999999]
["2008-06-11",2.91,2.81,1029.22,1029.26]
["2008-09-24",3.36,3.25,1028.7700000000002,1028.82]
["2009-06-29",4.17,4.04,1027.96,1028.03]
["2009-09-30",2.9710000000000001,2.87,{"$f":"F$3+F$1-B53","v":1029.1590000000001},{"$f":"F$3+F$2-C53","v":1029.2}]
["2010-05-15",2.9540000000000002,2.8530000000000002,{"$f":"F$3+F$1-B54","v":1029.1760000000002},{"$f":"F$3+F$2-C54","v":1029.2169999999999}]
["2010-06-02",3.3919999999999999,3.282,{"$f":"F$3+F$1-B55","v":1028.7380000000001},{"$f":"F$3+F$2-C55","v":1028.788}]
["2010-09-10",5.51,3.7650000000000001,{"$f":"F$3+F$1-B56","v":1026.6200000000001},{"$f":"F$3+F$2-C56","v":1028.3049999999998}]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]

{"sheet":"96-4(ABC&D)(TH-45)","index":16,"n_rows":58,"n_cols":18,"rows_kept":58,"cut":false,"hidden":false,"merged":[[57,0,57,9],[0,2,0,3],[2,2,2,3],[0,8,0,9],[1,8,1,9],[2,8,2,9],[0,4,0,5],[1,4,1,5],[2,4,2,5],[2,6,2,7],[5,0,6,0],[5,9,6,9],[1,2,1,3],[0,0,1,1],[5,1,5,4],[0,6,0,7],[5,5,5,8],[3,8,3,9],[4,8,4,9],[3,6,3,7],[4,6,4,7],[3,2,3,3],[4,2,4,3],[3,4,3,5],[4,4,4,5],[1,6,1,7]]}
["BH96-4",null,"Location:",null,"Intermediate Dam Toe, \nnear South Abutment",null,"2004 Stick Up - A (m):",null,0.95,null,null,"Standpipe","Tip Elevation"]
[null,null,"Coordinates:",null,"8V580669 \n6914113",null,"2004 Stick Up - B (m):",null,0.87,null,null,"a",{"$f":"$I$5-6.48","v":1025.68}]
["Surface Protector:","N/A","Date Installed:",null,1996,null,"2004 Stick Up - C (m):",null,0.91,null,null,"b",{"$f":"I5-11.3","v":1020.8600000000001}]
["Screened Interval - A (m bgs):","5.7-6.48","Screened Interval - C \n(m bgs):",null,"14.97-16.47",null,"2004 Stick Up - D (m):",null,0.88,null,null,"c",{"$f":"I5-16.47","v":1015.69}]
["Screened Interval - B (m bgs):","9.8-11.3","Screened Interval - D \n(m bgs):",null,"26.84-28.34",null,"2004 Surface \nElevation (m amsl):",null,1032.1600000000001,null,null,"d",{"$f":"I5-28.34","v":1003.82}]
["Date","Water level from top of pipe                                                                                                    (m)",null,null,null,"Piezometric Elevation                                                                                                                                                  (m amsl)",null,null,null,"Comments",null,null,null,"Ground Surface","tip A","tip B","tip C","tip D"]
[null,"A","B","C","D","A","B","C","D",null,null,null,"1996-01-01",1032.1600000000001,1025.68,1020.86,1015.69,1003.82]
["1996-09-08",3.11,3.04,2.98,2.88,1029.99,1030.01,1030.02,1030.1199999999999,null,null,null,"2012-12-31",1032.1600000000001,1025.68,1020.86,1015.69,1003.82]
["1996-09-26",3.27,3.25,3.12,3.05,1029.83,1029.8,1029.8800000000001,1029.95]
["1996-09-27"]
["1997-05-13",5.21,null,4.8499999999999996,null,1027.8900000000001,null,1028.1500000000001]
["1997-06-06"]
["1997-07-11",null,3.51,null,null,null,1029.54]
["1997-10-07",1.45,1.87,1.82,null,1031.6500000000001,1031.18,1031.18]
["1998-06-01",1.84,1.84,1.83,1.62,1031.26,1031.21,1031.17,1031.3800000000001]
["1998-10-31",3.18,3.15,3.09,3.01,1029.92,1029.9000000000001,1029.9100000000001,1029.99]
["1998-11-13"]
["1999-06-08"]
["1999-06-19",1.43,1.38,1.36,1.25,1031.67,1031.67,1031.6400000000001,1031.75]
["1999-07-03"]
["1999-10-29",3.68,3.62,3.6,3.48,1029.42,1029.43,1029.4000000000001,1029.52]
["1999-10-31"]
["2000-05-31"]
["2000-06-27",3.14,3.08,3.07,2.93,1029.96,1029.97,1029.93,1030.07]
["2000-07-25",null,null,2.84,null,null,null,1030.1600000000001]
["2000-09-21"]
["2000-10-10",2.92,2.85,2.83,2.71,1030.18,1030.2,1030.17,1030.29]
["2001-06-06",3.13,3.04,3.06,2.94,1029.97,1030.01,1029.94,1030.06]
["2001-07-15"]
["2001-09-05",2.77,2.68,2.71,2.57,1030.33,1030.3699999999999,1030.29,1030.43]
["2002-06-18",1.06,0.77,null,null,1032.04,1032.28]
["2002-08-05"]
["2002-09-10",3.3050000000000002,3.2349999999999999,3.25,3.105,1029.7950000000001,1029.8150000000001,1029.75,1029.895]
["2002-11-04"]
["2002-11-10"]
[{"$f":"'96-3(A&B)(TH-44)'!A36","v":"2003-06-11"},3.24,3.15,3.21,3.06,1029.8599999999999,1029.9000000000001,1029.79,1029.94]
[{"$f":"'96-3(A&B)(TH-44)'!A37","v":"2003-09-10"},4.1900000000000004,3.82,4.1500000000000004,3.99,1028.9100000000001,1029.23,1028.8499999999999,1029.01]
["2004-05-10",3.18,3.0950000000000002,3.14,3.01,{"$f":"$I$5+I$1-B38","v":1029.93},{"$f":"$I$5+I$2-C38","v":1029.9349999999999},{"$f":"$I$5+I$3-D38","v":1029.93},{"$f":"$I$5+I$4-E38","v":1030.0300000000002},"2004 survey info used from here on"]
["2004-07-08",3.1640000000000001,3.09,3.1150000000000002,2.9849999999999999,1029.9460000000001,1029.94,{"$f":"$I$5+I$3-D39","v":1029.9550000000002},1030.0550000000003]
["2004-07-19",3.56,3.09,3.1150000000000002,2.9849999999999999,1029.5500000000002,1029.94,{"$f":"$I$5+I$3-D40","v":1029.9550000000002},1030.0550000000003]
["2004-09-09",3.41,3.41,3.5,3.375,1029.7,1029.6199999999999,{"$f":"$I$5+I$3-D41","v":1029.5700000000002},1029.6650000000002,"a, b and c - dirty; d - clear; a and d - sulphur smell"]
["2005-05-26",4.415,3.74,null,4.2149999999999999,1028.6950000000002,1029.29,null,1028.8250000000003,"coarse sand frozen"]
["2005-09-14",5.0999999999999996,3.75,5.25,4.8899999999999997,1028.0100000000002,1029.28,{"$f":"$I$5+I$3-D43","v":1027.8200000000002},1028.1500000000001,"b- bottom blocked"]
["2006-03-09",5.5,"blocked",5.33,5.31,1027.6100000000001,null,{"$f":"$I$5+I$3-D44","v":1027.7400000000002},1027.7300000000002,"b- bottom blocked"]
["2006-03-27",5.19,"blocked",5.1150000000000002,4.99,1027.92,null,{"$f":"$I$5+I$3-D45","v":1027.9550000000002},1028.0500000000002,"b- bottom blocked, ice crystals on probe"]
["2006-06-14",2.66,3.75,0.4,4.9800000000000004,null,1028.4100000000001,null,1028.0600000000002,"b-bottom. C-bottom fine sand"]
["2006-10-02",5.28,3.75,5.2,5.07,1027.8300000000002,1028.4100000000001,{"$f":"$I$5+I$3-D47","v":1027.8700000000001},1027.9700000000003]
["2007-05-22",3.15,3.75,1.52,3.11,{"$f":"$I$5+I$1-B48","v":1029.96},1028.4100000000001,1031.5500000000002,{"$f":"$I$5+I$4-E48","v":1029.9300000000003},"a, b and d- frozen no beep"]
["2007-09-26",4.915,3.74,4.84,4.7050000000000001,1028.1950000000002,1028.42,1028.2300000000002,1028.3350000000003,"b: dry"]
["2008-05-20",3.46,3.37,3.39,2.6,1029.6500000000001,1028.7900000000002,1029.68,1030.4400000000003]
["2008-06-11",3.79,3.7,3.72,3.6,1029.3200000000002,1028.46,1029.3500000000001,1029.4400000000003]
["2008-09-24",4.2300000000000004,3.75,4.1500000000000004,4.01,{"$f":"$I$5+I$1-B52","v":1028.8800000000001},1028.4100000000001,1028.92,1029.0300000000002,"b: dry"]
["2009-06-29",5.03,3.77,4.93,4.8,1028.0800000000002,1028.3900000000001,1028.1400000000001,1028.2400000000002,"b: no beep"]
["2009-09-30",3.851,3.77,3.7730000000000001,2.6520000000000001,1029.259,1028.3900000000001,{"$f":"$I$5+I$3-D54","v":1029.2970000000003},{"$f":"$I$5+I$4-E54","v":1030.3880000000001}]
["2010-05-15",null,null,null,3.6560000000000001,null,null,null,{"$f":"$I$5+I$4-E55","v":1029.3840000000002}]
["2010-06-02",null,null,null,4.0759999999999996,null,null,null,{"$f":"$I$5+I$4-E56","v":1028.9640000000002}]
["2010-09-10",null,null,null,5.2850000000000001,null,null,null,{"$f":"$I$5+I$4-E57","v":1027.7550000000001}]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]

{"sheet":"P01-03A(TH-46)","index":18,"n_rows":31,"n_cols":13,"rows_kept":31,"cut":false,"hidden":false,"merged":[[0,0,1,1],[30,0,30,5]]}
["P01-03",null,"Location:","Intermediate Dam Toe","2004 Stick-Up (m):",0.61]
[null,null,"Coordinates:","8V580636 \n6914064","2004 Surface \nElevation ( m amsl):",1031.52]
["Surface Protector:","yes","Date Installed:",1996,"Tip Elevation\n(m amsl):",1022.3520000000001]
[null,null,null,null,"Screened Interval\n(m bgs):","7.78 - 9.30",null,null,null,null,"Ground Surface","Bottom of Slotted Section","Top of Slotted Section"]
["Date",null,"Water level from top of pipe (m)","Piezometric Elevation                             (m amsl)","Pond El. \n(m amsl)","Comments",null,null,null,"2000-09-01",1031.52,{"$f":"F2-9.17","v":1022.35},{"$f":"F2-7.65","v":1023.87}]
["2001-09-11",null,1.58,1030.6320000000001,null,null,null,null,null,"2012-12-31",1031.52,{"$f":"L5","v":1022.35},{"$f":"M5","v":1023.87}]
["2002-06-10",null,2.39,1029.8219999999999]
["2002-09-23",null,2.06,1030.152,{"$f":"1079.487-32.3","v":1047.1870000000001},null,null,null,null,36770]
["2003-06-11",null,1.61,1030.6020000000001,null,null,null,null,null,38353]
["2003-09-10",null,3.0750000000000002,1029.1369999999999]
["2004-05-10",null,1.7,{"$f":"F$2+F$1-C11","v":1030.4299999999998},null,"2004 survey info used from here on"]
["2004-07-08",null,1.82,1030.31]
["2004-07-19",null,2.0699999999999998,1030.06]
[{"$f":"'91-ID3(TH-37)'!A36","v":"2004-09-09"},null,2.4550000000000001,1029.675,null,"Dirty, strong sulphur smell"]
[{"$f":"'91-ID3(TH-37)'!A37","v":"2005-05-26"},null,3.2850000000000001,1028.8449999999998,null,"ph=6.7, temp=9.0C"]
[{"$f":"'91-ID3(TH-37)'!A38","v":"2005-09-14"},null,3.96,1028.1699999999998,null,"ph=6.8, temp=6.4C"]
["2006-03-09",null,4.38,1027.7499999999998]
["2006-03-27",null,4.07,1028.06]
["2006-06-14",null,4.0599999999999996,1028.07]
["2006-10-02",null,4.1399999999999997,1027.9899999999998]
["2007-05-22",null,2.4449999999999998,{"$f":"F$2+F$1-C21","v":1029.6849999999999},1046.7809999999999,"No Beep, frozen"]
["2007-09-26",null,4.01,1028.1199999999999,1047.7809999999999]
["2008-05-20",null,1.85,1030.28,null,"No Beep, frozen"]
["2008-06-11",null,2.71,1029.4199999999998]
["2008-09-24",null,3.1150000000000002,1029.0149999999999]
["2009-06-29",null,3.92,1028.2099999999998,1046.48]
["2009-09-30",null,2.7559999999999998,{"$f":"F$2+F$1-C27","v":1029.3739999999998},1046.048]
["2010-05-15",null,2.766,{"$f":"F$2+F$1-C28","v":1029.3639999999998},1046.269]
["2010-06-02",null,3.1869999999999998,{"$f":"F$2+F$1-C29","v":1028.943},1045.94]
["2010-09-10",null,4.3949999999999996,{"$f":"F$2+F$1-C30","v":1027.7349999999999},1043.7260000000001]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]

{"sheet":"P01-04(A&B)(Th-47)","index":20,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[[32,0,32,5],[0,0,1,1],[5,5,6,5],[5,0,6,0],[5,1,5,2],[5,3,5,4]]}
["P01-04",null,"Location:","Intermediate Dam Toe","2004 Stick Up - A (m): ",0.45]
[null,null,"Coordinates:","8V580489 \n6913888","2004 Stick Up -B (m): ",0.45]
["Surface Protector:","yes","Date Installed:",1996,"2004 Surface \nElevation ( m amsl):",1032.32]
[null,null,"Screened Interval -A (m bgs):","31.7 - 33.22","Tip Elevation - A\n(m amsl):",998.17,null,null,null,"Ground Surface","Bottom of Slotted Section (A)","Bottom of Slotted Section (B)"]
[null,null,"Screened Interval - B (m bgs):","51.0 - 52.5","Tip Elevation - B\n(m amsl):",978.89,null,null,"2001-01-01",{"$f":"F3","v":1032.32},998.17,978.89]
["Date","Water level from top of pipe                                                         (m)",null,"Piezometric Elevation\n(m amsl)",null,"Comments",null,null,"2010-12-31",{"$f":"F3","v":1032.32},998.17,978.89]
[null,"A","B","A","B"]
["2001-09-11",0.78,0.43,1031.1199999999999,1031.46]
["2002-06-10",1.67,1.29,1030.23,1030.5999999999999]
["2002-09-23",1.39,1,1030.51,1030.8900000000001]
[{"$f":"'P01-03A(TH-46)'!A9","v":"2003-06-11"},1.45,1.03,1030.45,1030.8599999999999,null,null,null,36892]
[{"$f":"'P01-03A(TH-46)'!A10","v":"2003-09-10"},2.35,1.9,1029.55,1029.99]
["2004-05-10",1.25,1.17,{"$f":"$F$3+$F$1-B13","v":1031.52},{"$f":"$F$3+$F$2-C13","v":1031.5999999999999},"2004 survey info used from this point on"]
["2004-07-08",1.18,0.755,1031.5899999999999,1032.0149999999999]
["2004-07-19",1.42,0.99,1031.3499999999999,1031.78]
[{"$f":"'91-ID3(TH-37)'!A36","v":"2004-09-09"},1.825,1.4,1030.9449999999999,1031.3699999999999]
[{"$f":"'91-ID3(TH-37)'!A37","v":"2005-05-26"},0.53,0.6,1032.24,1032.17,"bottom, no beep"]
[{"$f":"'91-ID3(TH-37)'!A38","v":"2005-09-14"},2.69,3.2149999999999999,1030.08,1029.5550000000001]
["2006-03-09",1.99,3.71,1030.78,1029.06]
["2006-03-27",1.99,3.42,1030.78,1029.3499999999999,"bottom "]
["2006-06-14",1.9850000000000001,2.5950000000000002,1030.7850000000001,1030.175,"bottom"]
["2006-10-02",2.85,3.4,1029.92,1029.3699999999999]
["2007-05-22",0.82,2.13,{"$f":"$F$3+$F$1-B23","v":1031.95},{"$f":"$F$3+$F$2-C23","v":1030.6399999999999},"a-beep, b-frozen no beep"]
["2007-09-26",2.4449999999999998,3,1030.325,1029.77]
["2008-05-20",0.68500000000000005,1.56,1032.085,1031.21,"b-no beep, frozen"]
["2008-06-11",1.39,1.93,1031.3799999999999,1030.8399999999999]
["2008-09-24",1.645,2.2599999999999998,1031.125,1030.51]
["2009-06-29",2.44,3.04,1030.33,1029.73]
["2009-09-30",1.365,1.845,{"$f":"$F$3+$F$1-B29","v":1031.405},{"$f":"$F$3+$F$2-C29","v":1030.925}]
["2010-05-15",1.595,2.0409999999999999,{"$f":"$F$3+$F$1-B30","v":1031.175},{"$f":"$F$3+$F$2-C30","v":1030.729}]
["2010-06-02",1.7789999999999999,2.052,{"$f":"$F$3+$F$1-B31","v":1030.991},{"$f":"$F$3+$F$2-C31","v":1030.7180000000001}]
["2010-09-10",3.5,2.95,{"$f":"$F$3+$F$1-B32","v":1029.27},{"$f":"$F$3+$F$2-C32","v":1029.82}]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]

{"sheet":"BKS04-06(TH-48)","index":22,"n_rows":22,"n_cols":13,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,1,1],[21,0,21,5]]}
["BKS04-06",null,"Location:","Intermediate Dam South Abutment","2004 Stick-Up (m):",1.5081199999999999]
[null,null,"Coordinates:","N 6913803\nE 580454.9","Tip Elevation\n(m amsl):",1036]
["Surface Protector:","yes","Date Installed:",1996,"2004 Surface \nElevation ( m amsl):",1049.0999999999999]
[null,null,null,null,"Screened Interval\n(m bgs):","12.8 - 13.1",null,null,null,null,"Ground Surface","Bottom of Slotted Section","Top of Slotted Section"]
["Date","Water level from top of pipe (m)",null,"Piezometric Elevation                             (m amsl)","Pond El. \n(m amsl)","Comments",null,null,null,"2003-01-01",1049.0999999999999,1036,1036.3]
["2005-05-26",13.01,null,{"$f":"$F$3+$F$1-B6","v":1037.5981199999999},null,null,null,null,null,"2011-12-31",1049.0999999999999,1036,1036.3]
["2005-09-14",14.15,null,1036.4581199999998,null,"bottom - no beep"]
["2006-03-09",13.87,null,1036.73812]
["2006-03-27",13.035,null,1037.5731199999998,null,"no beep"]
["2006-06-14",14.14,null,1036.4681199999998,null,"sticky at 11.0m"]
["2006-10-02",14.11,null,1036.49812]
["2007-05-22",13.855,null,{"$f":"$F$3+$F$1-B12","v":1036.7531199999999},1046.7809999999999,"Bottom no beep "]
["2007-09-26",14.15,null,{"$f":"$F$3+$F$1-B13","v":1036.4581199999998},null,"no beep"]
["2008-05-20",1.82,null,null,null,"no beep"]
["2008-06-11",1.79,null,null,null,"no beep"]
["2008-09-24",14.16,null,{"$f":"$F$3+$F$1-B16","v":1036.4481199999998},null,"no beep"]
["2009-06-29",14.164999999999999,null,1036.4431199999999,null,"beeped"]
["2009-09-30",14.265000000000001,null,1036.3431199999998,null,"no beep"]
["2010-05-15",1.9350000000000001,null,null,1046.269,"Stuck in slush; No beep"]
["2010-06-02",14.17,null,1036.4381199999998,1045.94]
["2010-09-10",13.875,null,null,1043.7260000000001,"Stuck in slush; No beep"]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]

{"sheet":"BKS04-07(TH-49)","index":24,"n_rows":22,"n_cols":13,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,1,1],[21,0,21,5]]}
["BKS04-07",null,"Location:","Intermediate Dam \nSouth Abutment","2004 Stick-Up (m):",1.51]
[null,null,"Coordinates:","N 6913747\nE 580407.6","Tip Elevation\n(m amsl):",1037.29]
["Surface Protector:","yes","Date Installed:",1996,"2004 Surface \nElevation ( m amsl):",1049.2]
[null,null,null,null,"Screened Interval\n(m bgs):","11.5 - 11.81",null,null,null,null,"Ground Surface","Bottom of Slotted Section","Top of Slotted Section"]
["Date",null,"Water level from top of pipe (m)","Piezometric Elevation                             (m amsl)","Pond El. \n(m amsl)","Comments",null,null,null,"2003-01-01",1049.2,1037.29,1037.5999999999999]
["2005-05-26",null,14.154999999999999,null,null,"Impossible reading",null,null,null,"2009-12-31",1049.2,1037.29,1037.5999999999999]
["2005-09-14",null,12.99,{"$f":"F$3+F$1-C7","v":1037.72}]
["2006-03-09",null,13.03,{"$f":"F$3+F$1-C8","v":1037.68}]
["2006-03-27",null,14.16,{"$f":"F$3+F$1-C9","v":1036.55},null,"no beep"]
["2006-06-14",null,13.02,{"$f":"F$3+F$1-C10","v":1037.69},null,"sticky at 12.7 m"]
["2006-10-02",null,13.01,{"$f":"F$3+F$1-C11","v":1037.7}]
["2007-05-22",null,2.0299999999999998,null,1046.7809999999999,"no beep, frozen"]
["2007-09-26",null,13.025,{"$f":"F$3+F$1-C13","v":1037.6849999999999},1047.7809999999999]
["2008-05-20",null,1.99,null,null,"no beep"]
["2008-06-11",null,2.89,null,null,"no beep"]
["2008-09-24",null,13.404999999999999,{"$f":"F$3+F$1-C16","v":1037.3050000000001}]
["2009-06-29",null,3.58,null,null,"blocked"]
["2009-09-30",null,13.053000000000001,{"$f":"F$3+F$1-C18","v":1037.6569999999999},1046.048]
["2010-05-15",null,13.081,{"$f":"F$3+F$1-C19","v":1037.6290000000001},1046.269]
["2010-06-02",null,null,null,1045.94,"Hit something solid - either ground or ice."]
["2010-09-10",null,12.785,{"$f":"F$3+F$1-C21","v":1037.925},1043.7260000000001,"Hit something solid - probably ground; No beep."]
["Note: Data until end of 2009 as compiled in BGC 2009 Annual Geotechnical Evaluation and Instrumentation Review; \n2010 Data compiled by DES"]