Publication information

Geological Survey of Canada
Open File 8885

Geomorphic feature inventory along the Dempster and Inuvik to Tuktoyaktuk highway corridor, Yukon and Northwest Territories

W.E. Sladen, R.J.H. Parker, P.D. Morse, S.V. Kokelj, and S.L. Smith

© Her Majesty the Queen in Right of Canada, as represented by the Minister of Natural Resources, 2022

Permanent link: https://doi.org/10.4095/329969

Publications in this series have not been edited; they are released as submitted by the author.

Recommended citation

Sladen, W.E., Parker, R.J.H., Morse, P.D., Kokelj, S.V., and Smith, S.L., 2022. Geomorphic feature inventory along the Dempster and Inuvik to Tuktoyaktuk highway corridor, Yukon and Northwest Territories; Geological Survey of Canada, Open File 8885, 1 .zip file. https://doi.org/10.4095/329969

System requirements

PC with 486 or greater processor, or Mac® with OS® X v. 10.2.2 or later; Adobe® Reader® v. 6.0 or later; video resolution of 1280 x 1024.

Trademarks

Adobe®, Acrobat®, and Reader® are either registered trademarks or trademarks of Adobe Systems Incorporated in the United States and/or other countries.

ESRI®, ArcExplorer™ and ArcReader™ are trademarks, registered trademarks, or service marks of ESRI® in the United States, the European Community, or certain other jurisdictions.

Contents

This multi-component Open File contains a report and georeferenced digital data in comma separated value (CSV) format, compressed Keyhole Markup Language (KML) with .kmz file extension format, and shapefile (SHP) format.

Directory structure

of_8885_readme.rtf (this file)
of_8885.pdf (report)
\Data		- Contains directories of digital data in multiple formats.
        \CSV	- Contains a comma separated value (csv) file for each feature class.
        \KML	- Contains a compressed Keyhole Markup Language (kmz) file for each feature class.
        \SHP	- Contains a shapefile (shp) for each feature class.

Projection Description

Projected Coordinate System: NAD_1983_UTM_Zone_8N
Projection: Transverse Mercator
False Easting: 500000.000000
False Northing: 0.000000
Central Meridian: -135.000000
Scale Factor: 0.999600
Latitude of Origin: 0.000000
Linear Unit: Meter (1.000000)

Geographic Coordinate System: GCS_North_American_1983
Angular Unit: Degree
Prime Meridian: Greenwich
Datum: D_North_American_1983

Topographic Data from Natural Resources Canada

Author contact information

W.E. Sladen (wendy.sladen@nrcan-rncan.gc.ca)
Geological Survey of Canada
601 Booth Street
Ottawa, Ontario
K1A 0E8

Availability information

This publication is available for free download through GEOSCAN (https://geoscan.nrcan.gc.ca/).

Terms of use

Information contained in this publication or product may be reproduced, in part or in whole, and by any means, for personal or public non-commercial purposes, without charge or further permission, unless otherwise specified.
You are asked to:
•	exercise due diligence in ensuring the accuracy of the materials reproduced;
•	indicate the complete title of the materials reproduced, and the name of the author organization; and
•	indicate that the reproduction is a copy of an official work that is published by Natural Resources Canada (NRCan) and that the reproduction has not been produced in affiliation with, or with the endorsement of, NRCan.
Commercial reproduction and distribution is prohibited except with written permission from NRCan. For more information, contact NRCan at copyright-droitdauteur@nrcan-rncan.gc.ca.

Terms of use for data

View the licence agreement for data at http://open.canada.ca/en/open-government-licence-canada